|  |  |  |
| --- | --- | --- |
| **THIS FORM IS A LEGAL REQUIREMENT OF THE BRITISH HEALTH & SAFETY REGULATIONS. CONTROL OF SUBSTANCES HAZARDOUS TO HEALTH (COSHH).** | | |
| Customer: | Contact Name: | |
| Return Address: | Contact No.: | |
| Purchase Order No.: | |
| Instrument: | Serial No.: | |
| Diameter: | Process Connection: | |
| **CALIBRATION AND TEST INFORMATION** | | |
| Meter Flow Range: l/s  l/min  l/hr  m3/hr  Other: | | |
| Meter Power Supply: 8V DC  12-24V DC  110/240V AC  N/A | | |
| Meter to be tested using: Pulse Output  4-20mA Output  Display Only | | |
| Calibration Points Required: 3  5  7  10  Repeats: 1  2  3 | | |
| Calibration Data Required: Flow Rates c/w mA Values  Flow Rates c/w Frequency (Hz)  *If unsure, tick ‘Error Only’* Pulses Collected  Average K-factor  Error Only (%) | | |
| **COSHH INFORMATION** | | |
| What liquid has the flowmeter been measuring? | | |
| Is the unit clean and free of all contaminants? YES  NO | | |
| Is the unit safe to handle? YES  NO | | |
| Method of cleaning: | | |
| Precautions to be taken: | | |
| Signature: | | Date: |
| Name:  *Please print* | | Position: |
| Please note that meters MUST be returned clean and certified to be free of any oil, chemical or toxic contaminants. Equipment received without COSHH clearance will be quarantined until a certificate declaring the instrument as clean and contaminant free has been received. | | |
| PLEASE EMAIL BACK TO:  [**info@flowhire.co.uk**](mailto:info@flowhire.co.uk)  Registered No. 03488133 ENGLAND & WALES  Directors: MJ Bancroft, LE Wood, CS Naylor, P Casson | | |

A blue and black logo

Description automatically generated

**COSHH Clearance Form**

**Riverside, Canal Road, Sowerby Bridge, HX6 2AY**