|  |
| --- |
| **THIS FORM IS A LEGAL REQUIREMENT OF THE BRITISH HEALTH & SAFETY REGULATIONS. CONTROL OF SUBSTANCES HAZARDOUS TO HEALTH (COSHH).** |
| Customer: | Contact Name:  |
| Return Address: | Contact No.: |
| Purchase Order No.: |
| Instrument: | Serial No.: |
| Diameter: | Process Connection: |
| **CALIBRATION AND TEST INFORMATION** |
| Meter Flow Range: l/s [ ]  l/min [ ]  l/hr [ ]  m3/hr [ ]  Other:  |
| Meter Power Supply: 8V DC [ ]  12-24V DC [ ]  110/240V AC [ ]  N/A [ ]  |
| Meter to be tested using: Pulse Output [ ]  4-20mA Output [ ]  Display Only [ ]  |
| Calibration Points Required: 3 [ ]  5 [ ]  7 [ ]  10 [ ]  Repeats: 1 [ ]  2 [ ]  3 [ ]  |
| Calibration Data Required: Flow Rates c/w mA Values [ ]  Flow Rates c/w Frequency (Hz) [ ] *If unsure, tick ‘Error Only’* Pulses Collected [ ]  Average K-factor [ ]  Error Only (%) [ ]  |
| **COSHH INFORMATION** |
| What liquid has the flowmeter been measuring?  |
| Is the unit clean and free of all contaminants? YES [ ]  NO [ ]  |
| Is the unit safe to handle? YES [ ]  NO [ ]  |
| Method of cleaning:  |
| Precautions to be taken: |
| Signature: | Date: |
| Name:*Please print* | Position: |
| Please note that meters MUST be returned clean and certified to be free of any oil, chemical or toxic contaminants. Equipment received without COSHH clearance will be quarantined until a certificate declaring the instrument as clean and contaminant free has been received. |
| PLEASE EMAIL BACK TO:**info@flowhire.co.uk**Registered No. 03488133 ENGLAND & WALESDirectors: MJ Bancroft, LE Wood, CS Naylor, P Casson |



**COSHH Clearance Form**

**Riverside, Canal Road, Sowerby Bridge, HX6 2AY**